R1#ping 192.168.5.2

Type escape sequence to abort.

Sending 5, 100-byte ICMP Echos to 192.168.5.2, timeout is 2 seconds:

!!!!!

Success rate is 100 percent (5/5), round-trip min/avg/max = 1/1/4 ms

R1#ping 2001:db8:e::2

Type escape sequence to abort.

Sending 5, 100-byte ICMP Echos to 2001:DB8:E::2, timeout is 2 seconds:

!!!!!

Success rate is 100 percent (5/5), round-trip min/avg/max = 1/1/4 ms

R1#traceroute 192.168.5.2

Type escape sequence to abort.

Tracing the route to 192.168.5.2

VRF info: (vrf in name/id, vrf out name/id)

1 192.168.2.2 0 msec 0 msec 0 msec

2 192.168.3.2 0 msec 4 msec 0 msec

3 192.168.4.2 0 msec 0 msec 0 msec

4 192.168.5.2 4 msec \* 0 msec

R1#traceroute 2001:db8:e::2

Type escape sequence to abort.

Tracing the route to 2001:DB8:E::2

1 2001:DB8:B::2 0 msec 0 msec 0 msec

2 2001:DB8:C::2 0 msec 0 msec 4 msec

3 2001:DB8:D::2 0 msec 0 msec 0 msec

4 2001:DB8:E::2 4 msec 0 msec 0 msec