R5#ping 192.168.2.1

Type escape sequence to abort.

Sending 5, 100-byte ICMP Echos to 192.168.2.1, timeout is 2 seconds:

!!!!!

Success rate is 100 percent (5/5), round-trip min/avg/max = 1/1/4 ms

R5#ping 2001:db8:b::1

Type escape sequence to abort.

Sending 5, 100-byte ICMP Echos to 2001:DB8:B::1, timeout is 2 seconds:

!!!!!

Success rate is 100 percent (5/5), round-trip min/avg/max = 1/1/4 ms

R5#traceroute 192.168.2.1

Type escape sequence to abort.

Tracing the route to 192.168.2.1

VRF info: (vrf in name/id, vrf out name/id)

1 192.168.5.1 0 msec 0 msec 0 msec

2 192.168.4.1 0 msec 0 msec 0 msec

3 192.168.3.1 0 msec 0 msec 0 msec

4 192.168.2.1 0 msec 0 msec \*

R5#traceroute 2001:db8:b::1

Type escape sequence to abort.

Tracing the route to 2001:DB8:B::1

1 2001:DB8:E::1 0 msec 0 msec 0 msec

2 2001:DB8:D::1 0 msec 0 msec 0 msec

3 2001:DB8:C::1 0 msec 0 msec 0 msec

4 2001:DB8:B::1 0 msec 0 msec 0 msec